{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Page1-版本记录","Page2-进迭严控物料（DDR、EMMC）","Page3-立项推荐物料"],"not_rendered":{"charts":0,"images":5,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Page1-版本记录","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
[null,"日期\nDate","版本\nVersion","更新点\nUpdate Highlights","备注\nNotes"]
[null,20240402,"V1.0","新增page3 型号明细\nAdd a new Page 3 for the detailed model list."]
[null,20240415,"V1.1","增加LPDDR4X AVL型号\nAdd LPDDR4X AVL models"]
[null,20240426,"V1.2","增加其他已适配外设型号\nAdd other peripheral models that have been adapted."]
[null,20240511,"V1.3","修改AVL格式，删除测试不完善的物料型号\nUpdate the AVL format and eliminate part numbers that have not passed complete testing."]
[null,20240520,"V1.4","增加DDR和EMMC可支持型号\nRevise the AVL format to remove material models that have not been fully tested."]
[null,20240613,"V1.5","增加DDR和EMMC可支持型号\nAdd supported models for DDR and eMMC"]
[null,20240708,"V1.6","暂时移除江波龙8GB LPDDR4x型号，补充信号测试\nTemporarily remove the 8GB LPDDR4x model from Longsys, and conduct additional signal testing."]
[null,20240711,"V1.7","1.增加支持256GB 江波龙、128GB 闪迪、256GB 佰维EMMC物料\n2.江波龙8GB LPDDR4x型号，信号测试PASS，重新加入AVL\n3.增加支持codec芯片 ES8316\n1. Add support for 256GB Longsys, 128GB SanDisk, and 256GB Biwin eMMC materials.\n2. The 8GB LPDDR4x model from Longsys has passed the signal test and is re-added to the AVL.\n3. Add support for the codec chip ES8316."]
[null,20240815,"V1.8","增加支持8GB 晶存、4GB长鑫、8GB长鑫 LPDDR4x物料\nAdd support for 8GB Jinding, 4GB CXMT, and 8GB CXMT LPDDR4x components."]
[null,20241028,"V1.9","1.修改Camera支持列表类型，新增Camera型号\n2.新增2款EMMC支持型号\n3.新增6款DDR支持型号\n1. Modify the Camera support list type and add new Camera models.\n2. Add two new supported eMMC models.\n3. Add six new supported DDR models."]
[null,20241101,"V2.0","1.DDR支持列表，增加一列\"SDK最低版本\"\n2.补充“Page8-other” sheet，已支持物料\n1. Add a column \"Minimum SDK Version\" to the DDR support list.\n2. Supplement the \"Page8-other\" sheet with supported materials."]
[null,20250221,"V2.1","更新DDR支持型号\nUpdate the supported DDR models"]
[null,20250403,"V2.2","1.调整AVL表格格式，梳理进迭严控物料和立项推荐物料。并明确外设物料使用说明\n2.新增立项推荐物料\n1. Adjust the AVL table format to organize the iterative strict control materials and recommended materials for project initiation. Clarify the usage instructions for peripheral materials.\n2. Add new recommended materials for project initiation."]
[null,20250530,"V2.3","1.增加DDR、EMMC物料量产状态\n2.更新Camera型号\n3.增加EMMC适配型号\n1. Add the production status of DDR and eMMC materials.\n2. Update the Camera models.\n3. Add new eMMC adaptation models."]
[null,20250709,"V2.4","新增英语描述\nAdd English Description"]
[null,20250822,"V2.5","1.更新ES8388停产计划\nUpdated ES8388 end-of-life (EOL) plan"]
[null,20251119,"V2.6","1.增加华邦1GB和512MB的LPDDR4x颗粒（仅用于-20~70℃场景）\n2.增加宏芯宇64GB EMMC颗粒、晶存32GB EMMC颗粒\n3.增加金士顿16GB EMMC颗粒\n1. Added Winbond 1GB and 512MB LPDDR4x components (for –20°C to +70°C applications only)\n2. Added MXCY 64GB eMMC and Jingcun 32GB eMMC components\n3. Added Kingston 16GB eMMC component"]

{"sheet":"Page2-进迭严控物料（DDR、EMMC）","index":1,"n_rows":50,"n_cols":10,"rows_kept":50,"cut":false,"hidden":false,"merged":[[6,0,26,0],[30,0,49,0],[6,1,18,1],[19,1,26,1],[30,1,40,1],[41,1,49,1],[0,0,4,9]]}
["注意：使用下表中的LPDDR4x、EMMC物料，进迭对技术问题负责；\n不在下表中的LPDDR4x、EMMC物料，进迭视具体案例决定是否提供技术支持，不对技术问题负责。\n\nNote: SpacemiT assumes responsibility for technical issues related to LPDDR4x and eMMC components listed in the table below. For components not listed, technical support will be determined on a case-by-case basis, and SpacemiT shall not be held accountable for any technical issues."]
[]
[]
[]
[]
[]
["推荐物料\nRecommended Materials","LPDDR4X","序号\nSerial Number","型号\nModel","容量(GB)\nCapacity (GB)","CS-num","温度(℃)\nTemperature (℃)","厂家\nManufacturer","SDK最低版本\nMinimum SDK Version","量产状态\nProduction Status"]
[null,null,1,"CXDB5CBAM-MA-B","4GB",1,"-25-85","长鑫\nCXMT","v2.0","MP"]
[null,null,2,"CXDB6CCBM-MA-A","8GB",2,"-25-85","长鑫\nCXMT","v2.0","MP"]
[null,null,3,"CXDB7CCDM-MA-M","16GB",2,"-25-85","长鑫\nCXMT","v2.0","MP"]
[null,null,4,"BWCC2X32N2A-16G-X","2GB",1,"-25-85","佰维\nBiwin","v2.0","MP"]
[null,null,5,"BWCC2X32N2A-32G-X","4GB",2,"-25-85","佰维\nBiwin","v2.0","MP"]
[null,null,6,"BWMZCX32H2A-64G-X","8GB",2,"-25-85","佰维\nBiwin","v2.0","MP"]
[null,null,7,"BWMZCX32H2A-64GI-X","8GB",2,"-40-95","佰维\nBiwin","v2.0","MP"]
[null,null,8,"FLXC4008G-30","8GB",2,"-25-85","江波龙\nLongsys","v2.0","MP"]
[null,null,9,"ATL4X2G32M1D-46WT","2GB",1,"-25-85","晶存\nRayson","v2.1","MP"]
[null,null,10,"ATL4X4G32M1D-46WT","4GB",2,"-25-85","晶存\nRayson","v2.1","MP"]
[null,null,11,"W66DP2RQQAGJ","1GB",1,"-20-70","华邦\nwinbond","v2.0","MP"]
[null,null,12,"W66CP2RQQAGJ","512MB",1,"-20-70","华邦\nwinbond","v2.0","MP"]
[null,"EMMC","序号\nSerial Number","型号\nModel","容量(GB)\nCapacity (GB)","温度(℃)\nTemperature (℃)","厂家\nManufacturer","量产状态\nProduction Status"]
[null,null,1,"FEMDNN128G-A3V01",128,"-25-85","江波龙\nLongsys","MP"]
[null,null,2,"FEMDNN256G-A3V01",256,"-25-85","江波龙\nLongsys","MP"]
[null,null,3,"BWCTAKL11X128G",128,"-25-85","佰维\nBiwin","MP"]
[null,null,4,"BWCTAKL21X256G",256,"-25-85","佰维\nBiwin","MP"]
[null,null,5,"HSEMSDS7D2B128G",128,"-25-85","海康威视\nHikvision","MP"]
[null,null,6,"HAC21-64G0BSAC",64,"-25-85","宏芯宇\nHosinglobal","MP"]
[null,null,7,"EMMC16G-MW28",16,"-25-85","金士顿\nKingston","MP"]
[]
[]
[]
["已适配物料\nAdapted Materials","LPDDR4X","序号\nSerial Number","型号\nModel","容量(GB)\nCapacity (GB)","CS-num","温度(℃)\nTemperature (℃)","厂家\nManufacturer","SDK最低版本\nMinimum SDK Version","量产状态\nProduction Status"]
[null,null,1,"MLXW8008G-X8","8GB",2,"-25-85","江波龙\nLongsys","v2.0","MP，25年底EOL\nMP, EOL at the end of 2025"]
[null,null,2,"K4UBE3D4AB-MGCL","4GB",2,"-25-85","三星\nSamsung","v1.0","MP"]
[null,null,3,"K4UCE3Q4AB-MGCL","8GB",2,"-25-85","三星\nSamsung","v1.0","MP"]
[null,null,4,"MT53E512M32D1ZW-046 WT:B","2GB",1,"-25-85","镁光\nMicron","v1.0","MP"]
[null,null,5,"MT53E1G32D2FW-046WT:C","4GB",1,"-25-85","镁光\nMicron","v1.0","MP"]
[null,null,6,"MT53D1024M32D4DT-046 WT:D","4GB",2,"-25-85","镁光\nMicron","v1.0","EOL"]
[null,null,7,"MT53E2G32D4DE-046WT:C","8GB",2,"-25-85","镁光","v1.0","MP"]
[null,null,8,"MT53E4G32D8CY-046 WT:C","16GB",2,"-25-85","镁光\nMicron","v1.0.7","MP"]
[null,null,9,"H9HCNNNCPMMLXR-NEE","4GB",2,"-25-85","海力士\nSK Hynix","v2.0","MP"]
[null,null,10,"H9HCNNNFAMMLXR-NEE","8GB",2,"-25-85","海力士\nSK Hynix","v2.1","MP"]
[null,"EMMC","序号\nSerial Number","型号\nModel","容量(GB)\nCapacity (GB)","温度(℃)\nTemperature (℃)","厂家\nManufacturer","量产状态\nProduction Status"]
[null,null,1,"FEMDNN064G-A3A55",64,"-25-85","江波龙\nLongsys","EOL"]
[null,null,2,"FEMDNN032G-A3A55",32,"-25-85","江波龙\nLongsys","EOL"]
[null,null,3,"FEMDNN016G-A3A55",16,"-25-85","江波龙\nLongsys","EOL"]
[null,null,4,"KLMAG1JETD-B041",16,"-25-85","三星\nSamsung","MP，26年Q1 EOL\nMP, EOL in Q1 2026"]
[null,null,5,"KLMBG2JETD-B041",32,"-25-85","三星\nSamsung","MP，26年Q1 EOL\nMP, EOL in Q1 2026"]
[null,null,6,"KLMCG4JETD-B041",64,"-25-85","三星\nSamsung","MP，26年Q1 EOL\nMP, EOL in Q1 2026"]
[null,null,7,"SDINBDA4-128G",128,"-25-85","闪迪\nSanDisk","EOL"]
[null,null,8,"RS70B32G4S15G",32,"-25-85","晶存\nRayson","MP"]

{"sheet":"Page3-立项推荐物料","index":2,"n_rows":80,"n_cols":10,"rows_kept":80,"cut":false,"hidden":false,"merged":[[15,2,15,9],[16,2,16,9],[17,2,17,9],[18,2,18,9],[19,2,19,9],[20,2,20,9],[21,2,21,9],[22,2,22,9],[6,0,9,0],[11,0,13,0],[15,0,47,0],[0,0,4,9]]}
["注意：下表物料，是进迭主控不同程度适配过的物料，立项时推荐优先选择，有利于项目产品规格目标的快速达成。使用推荐物料，进迭提供技术支持；不使用推荐物料，进迭视具体案例决定是否提供技术支持。\n\nNote: The materials listed in the table below have been adapted to varying degrees for SpacemiT SoCs and are recommended for priority selection at the project initiation stage. Choosing these recommended materials will help accelerate the achievement of product specification goals.\nSpacemiT will provide technical support for the recommended materials. For non-recommended materials, technical support will be determined on a case-by-case basis."]
[]
[]
[]
[]
[]
["SPI NOR","序号\nSerial Number","型号\nModel","容量(MB)\nCapacity (MB)","工作电压\nOperating Voltage","温度(℃)\nTemperature (℃)","厂家\nManufacturer"]
[null,1,"GD25Q64ESIG",8,"2.7~3.6V","-40-85","兆易创新\nGigaDevice"]
[null,2,"FM25Q64AI3",8,"2.7~3.6V","-40-85","复旦微电子\nFudan Microelectronics"]
[null,3,"W25Q64FWSSAQ",8,"1.65~1.95V","-25-105","华邦\nWinbond"]
[]
["EEPROM","序号\nSerial Number","型号\nModel","容量(Kbits)\nCapacity (Kbits)","工作电压\nOperating Voltage","温度(℃)\nTemperature (℃)","厂家\nManufacturer"]
[null,1,"GT24C02B-2TFLI-TR",2,"1.65~5.5V","-40-85","聚辰"]
[null,2,"FT24C02A-KLG-R",2,"1.8~5.5V","-40-85","辉芒微"]
[]
["Camera","适配状态\nAdaptation Status","描述\nDescription"]
[null,"X","不支持\nNot Supported"]
[null,"N/T","不确定\nUncertain"]
[null,"D/S","支持\nSupported"]
[null,"S/T","Sample通过出图测试\nSample passed the imaging test"]
[null,"I/Q","完成IQ调试\nCompleted IQ debugging"]
[null,"√","已量产\nIn mass production"]
[]
[null,"序号\nSerial Number","型号\nModel","像素\nPixels","接口\nInterface","位宽（bits）\nBit Width (bits)","帧率（fps）\nFrame Rate (fps)","已支持最大分辨率\nMaximum Supported Resolution","厂家\nManufacturer","适配状态\nAdaptation Status"]
[null,1,"GC2375","2M","MIPI CSI 1lane",10,30,"1600x1200","格科微\nGalaxyCore","I/Q"]
[null,2,"GC13A0","13M","MIPI CSI 4lane",10,30,"4208x3120","格科微\nGalaxyCore","I/Q"]
[null,3,"GC08A8","8M","MIPI CSI 4lane",10,30,"3264x2448","格科微\nGalaxyCore","I/Q"]
[null,4,"GC5035","5M","MIPI CSI 2lane",10,30,"2592x1944","格科微\nGalaxyCore","I/Q"]
[null,5,"GC2385","2M","MIPI CSI 1lane",10,"/","/","格科微\nGalaxyCore","D/S"]
[null,6,"S5K5E3YX","5M","MIPI CSI 2lane",10,30,"2560x1920","三星\nSamsung","I/Q"]
[null,7,"MLX75027","0.3M","MIPI CSI 2lane",12,120,"640x480","迈来芯\nMelexis","S/T"]
[null,8,"BF2257CS","2M","MIPI CSI 1lane",10,30,"1600x1200","比亚迪\nBYD","I/Q"]
[null,9,"IMX135","13M","MIPI CSI 4lane",10,30,"4208x3120","索尼\nSony","I/Q"]
[null,10,"IMX219","8M","MIPI CSI 4lane",10,30,"1920x1080","索尼\nSony","I/Q"]
[null,11,"IMX415","8M","MIPI CSI 4lane",10,30,"3864x2192","索尼\nSony","I/Q"]
[null,12,"SC031GS","0.3M","MIPI CSI 1lane",10,30,"640x480","思特威\nSmartSens","√"]
[null,13,"SC035HGS","0.3M","MIPI CSI 1lane",10,30,"640x480","思特威\nSmartSens","I/Q"]
[null,14,"SC501AI","5M","MIPI CSI 2lane",10,30,"2688x1616","思特威\nSmartSens","I/Q"]
[null,15,"OV5647","5M","MIPI CSI 2lane",10,15,"2592x1944","豪威\nOmnivision","I/Q"]
[null,16,"OG02B10","2M","MIPI CSI 2lane",10,60,"1600x1300","豪威\nOmnivision","S/T"]
[null,17,"OS05A10","2M","MIPI CSI 1lane",10,30,"1920x1080","豪威\nOmnivision","I/Q"]
[null,18,"OV08D10","8M","MIPI CSI 2lane",10,30,"3264x2448","豪威\nOmnivision","I/Q"]
[null,19,"OV13B10","13M","MIPI CSI 4lane",10,30,"4208x3120","豪威\nOmnivision","I/Q"]
[null,20,"OV16A10","16M","MIPI CSI 4lane",10,30,"3840x2160","豪威\nOmnivision","S/T"]
[null,21,"OV8856","8M","MIPI CSI 4lane",10,30,"2560x1440","豪威\nOmnivision","S/T"]
[null,22,"OV13855","13M","MIPI CSI 4lane",10,"/","/","豪威\nOmnivision","I/Q"]
[null,23,"OV13850","13M","MIPI CSI 4lane",10,30,"4224x3136","豪威\nOmnivision","I/Q"]
[null,24,"OV5670","5M","MIPI CSI 2lane",10,"/","/","豪威\nOmnivision","I/Q"]
[]
["分类\nCategory","分类\nClassification","物料描述\nMaterial Description","品牌\nBrand","数据手册\nDatasheet"]
["芯片\nChip","GPHY","芯片-RTL8211F-CG-封装 QFN40_5R00X5R00X0R90_T\nChip-RTL8211F CG Package QFN40_5R00X5R00X0R90_T","瑞昱\nREALTEK"]
["芯片\nChip","GPHY","芯片-YT8531CA\nChip-YT8531CA","裕太微电子\nYutai Microelectronics"]
["芯片\nChip","GPHY","芯片-RTL8111H\nChip-RTL8111H","瑞昱\nREALTEK"]
["芯片\nChip","2.5GPHY","芯片-RTL8156BG-CG\nChip-RTL8156BG-CG","瑞昱\nREALTEK"]
["芯片\nChip","2.5GPHY","芯片-RTL8125B\nChip-RTL8125B","瑞昱\nREALTEK"]
["芯片\nChip","Codec","芯片-ES8326B\nChip-ES8326B","顺芯\nShunxin"]
["芯片\nChip","Codec","芯片-ES8316\nChip-ES8316","顺芯\nShunxin"]
["芯片\nChip","Codec","芯片-ES8388\nChip-ES8388","顺芯\nShunxin","2026.12.31 EOL"]
["芯片\nChip","Charge","芯片-SC8886SQDER\nChip-SC8886SQDER","顺芯\nShunxin"]
["芯片\nChip","Charge","芯片-SGM41515\nChip-SGM41515","圣邦微\nSGMICRO"]
["芯片\nChip","Coulomb counter","芯片-CW2015CHBD\nChip-CW2015CHBD","赛微\nCellwise"]
["芯片\nChip","CC logic&Switch","芯片-ANX7447\nChip-ANX7447","硅谷数模\nAnalogix Semiconductor"]
["芯片\nChip","CC logic","芯片-HUSB239\nChip-HUSB239","慧能泰\nHuineng Tai"]
["芯片\nChip","MIPI TO EDP","芯片-LT8911EXB\nChip-LT8911EXB","龙讯\nLong News"]
["芯片\nChip","HDMI TO DP","芯片-LT6711A\nChip-LT6711A","龙讯\nLong News"]
["芯片\nChip","4 port USB3 HUB","芯片-VL817\nChip-VL817","威锋电子\nWeifeng Electronics"]
["芯片\nChip","4 port USB3 HUB","芯片-GL3523-QFN76\nChip-GL3523-QFN76","创惟\nGENESYS"]
["芯片\nChip","4 port USB2 HUB","芯片-GL850G\nChip-GL850G","创惟\nGENESYS"]
["芯片\nChip","PCIE TO SATA","芯片-JMB582\nChip-JMB582","智微\nJMicron"]
["芯片\nChip","PCIE TO SATA","芯片-ASM1061\nChip-ASM1061","祥硕\nASMedia"]
["模组\nModule","WIFI/BT","SDIO/UART模组-RTL8852BS\nSDIO/UART Module - RTL8852BS","瑞昱-中龙通\nRuiyu Zhonglongtong"]
["模组\nModule","WIFI/BT","PCIE/USB模组-RTL8852BE\nPCIE/USB module - RTL8852BE","瑞昱-欧智通/中龙通\nRuiyu Ouzhitong/Zhonglongtong"]
["模组\nModule","WIFI/BT","SDIO/UART模组-AIC8800D\nSDIO/UART Module - AIC8800D","爱科微\nAike Micro"]
["模组\nModule","WIFI/BT","SDIO/UART模组-AP6256\nSDIO/UART Module - AP6256","正基科技"]
["模组\nModule","4G","NL668-757S-10","广和通\nFibocom"]
["电池\nBattery","4800mAh 7.6V 双节电池\n4800mAh 7.6V Dual Cell Battery","U487091PV-2S1P","优特利\nYouteli"]
["LCD屏\nLCD Screen","10.1寸MIPIDSI屏","JL-M101N013-P12WU-M402632","京龙光电\nJinglong Optoelectronics"]
["LCD屏\nLCD Screen","10.95寸MIPIDSI屏\n10.1-Inch MIPIDSI Screen","TLCM-HJR110101D","恒久瑞电子\nHengjiu Rui Electronics"]
["LCD屏\nLCD Screen","8寸MIPIDSI屏\n8-Inch MIPIDSI Screen","JLT080KI26184P30-21D01","吉兰特科技\nJilante Technology"]
["LCD屏\nLCD Screen","14寸EDP屏\n14-Inch EDP Screen","ZTM140XXXE4505","正通仁禾科技\nZhengtong Renhe Technology"]